,Light Engine##OTHER##,Drive Current##OTHER##,LED Colour##OTHER##,Beam Angle##OTHER##,Finish##OTHER##,Model##OTHER##,Colour##OTHER##,Finish Material##OTHER##,MFG_CRI##OTHER##,MFG_LightSource##OTHER##,MFG_TemperatureRating##OTHER##,Control IES##OTHER##,MFG_Wattage##ELECTRICAL_WATTAGE##WATTS
E3 350mA 2200K NB Black GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-350-LW22-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2200K NB White GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-350-LW22-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2200K NB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW22-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2200K NB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW22-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2200K NB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW22-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2200K NB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW22-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2200K NB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-350-LW22-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2200K MB Black GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-350-LW22-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2200K MB White GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-350-LW22-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2200K MB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW22-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2200K MB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW22-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2200K MB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW22-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2200K MB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW22-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2200K MB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-350-LW22-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2200K WB Black GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-350-LW22-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2200K WB White GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-350-LW22-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2200K WB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW22-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2200K WB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW22-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2200K WB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW22-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2200K WB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW22-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2200K WB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-350-LW22-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2200K WWB Black GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-350-LW22-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2200K WWB White GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-350-LW22-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2200K WWB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW22-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2200K WWB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW22-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2200K WWB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW22-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2200K WWB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW22-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2200K WWB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-350-LW22-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2200K OB Black GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-350-LW22-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2200K OB White GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-350-LW22-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2200K OB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW22-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2200K OB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW22-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2200K OB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW22-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2200K OB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW22-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2200K OB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-350-LW22-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2700K NB Black GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-350-LW27-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2700K NB White GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-350-LW27-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2700K NB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW27-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2700K NB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW27-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2700K NB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW27-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2700K NB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW27-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2700K NB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-350-LW27-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 2700K MB Black GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-350-LW27-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2700K MB White GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-350-LW27-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2700K MB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW27-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2700K MB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW27-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2700K MB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW27-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2700K MB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW27-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2700K MB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-350-LW27-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 2700K WB Black GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-350-LW27-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2700K WB White GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-350-LW27-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2700K WB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW27-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2700K WB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW27-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2700K WB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW27-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2700K WB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW27-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2700K WB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-350-LW27-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 2700K WWB Black GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-350-LW27-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2700K WWB White GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-350-LW27-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2700K WWB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW27-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2700K WWB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW27-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2700K WWB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW27-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2700K WWB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW27-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2700K WWB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-350-LW27-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 2700K OB Black GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-350-LW27-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2700K OB White GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-350-LW27-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2700K OB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW27-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2700K OB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW27-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2700K OB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW27-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2700K OB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW27-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 2700K OB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-350-LW27-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 3000K NB Black GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-350-LW30-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 3000K NB White GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-350-LW30-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 3000K NB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW30-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 3000K NB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW30-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 3000K NB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW30-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 3000K NB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW30-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 3000K NB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-350-LW30-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 3000K MB Black GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-350-LW30-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 3000K MB White GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-350-LW30-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 3000K MB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW30-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 3000K MB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW30-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 3000K MB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW30-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 3000K MB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW30-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 3000K MB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-350-LW30-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 3000K WB Black GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-350-LW30-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 3000K WB White GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-350-LW30-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 3000K WB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW30-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 3000K WB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW30-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 3000K WB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW30-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 3000K WB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW30-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 3000K WB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-350-LW30-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 3000K WWB Black GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-350-LW30-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 3000K WWB White GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-350-LW30-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 3000K WWB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW30-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 3000K WWB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW30-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 3000K WWB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW30-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 3000K WWB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW30-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 3000K WWB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-350-LW30-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 3000K OB Black GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-350-LW30-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 3000K OB White GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-350-LW30-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 3000K OB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW30-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 3000K OB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW30-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 3000K OB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW30-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 3000K OB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW30-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 3000K OB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Warm White (3000K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-350-LW30-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 4000K NB Black GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-350-LW40-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 4000K NB White GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-350-LW40-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 4000K NB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW40-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 4000K NB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW40-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 4000K NB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW40-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 4000K NB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW40-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 4000K NB Custom RAL GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-350-LW40-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 4000K MB Black GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-350-LW40-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 4000K MB White GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,19° Medium,Powder Coat White (RAL 9016),LD10238-E3-350-LW40-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 4000K MB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW40-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 4000K MB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW40-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 4000K MB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW40-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 4000K MB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW40-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 4000K MB Custom RAL GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,19° Medium,Powder Coat RAL (TBD),LD10238-E3-350-LW40-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 4000K WB Black GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-350-LW40-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 4000K WB White GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,34° Wide,Powder Coat White (RAL 9016),LD10238-E3-350-LW40-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 4000K WB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW40-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 4000K WB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW40-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 4000K WB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW40-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 4000K WB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW40-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 4000K WB Custom RAL GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,34° Wide,Powder Coat RAL (TBD),LD10238-E3-350-LW40-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 4000K WWB Black GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-350-LW40-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 4000K WWB White GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-350-LW40-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 4000K WWB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW40-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 4000K WWB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW40-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 4000K WWB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW40-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 4000K WWB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW40-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 4000K WWB Custom RAL GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-350-LW40-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 4000K OB Black GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-350-LW40-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 4000K OB White GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-350-LW40-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 4000K OB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW40-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 4000K OB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW40-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 4000K OB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW40-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 4000K OB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW40-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 4000K OB Custom RAL GSA,E3 LED Engine,350mA (5W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-350-LW40-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 5000K NB Black GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-350-LW50-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 5000K NB White GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-350-LW50-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 5000K NB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW50-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 5000K NB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW50-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 5000K NB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW50-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 5000K NB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW50-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 5000K NB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-350-LW50-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-NB,4.4
E3 350mA 5000K MB Black GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-350-LW50-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 5000K MB White GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-350-LW50-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 5000K MB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW50-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 5000K MB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW50-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 5000K MB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW50-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 5000K MB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW50-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 5000K MB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-350-LW50-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-MB,4.4
E3 350mA 5000K WB Black GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-350-LW50-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 5000K WB White GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-350-LW50-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 5000K WB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW50-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 5000K WB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW50-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 5000K WB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW50-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 5000K WB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW50-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 5000K WB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-350-LW50-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WB,4.4
E3 350mA 5000K WWB Black GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-350-LW50-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 5000K WWB White GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-350-LW50-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 5000K WWB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW50-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 5000K WWB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW50-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 5000K WWB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW50-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 5000K WWB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW50-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 5000K WWB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-350-LW50-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-WWB,4.4
E3 350mA 5000K OB Black GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-350-LW50-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 5000K OB White GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-350-LW50-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 5000K OB Classic Bronze GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-350-LW50-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 5000K OB Textured Fir Green GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-350-LW50-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 5000K OB Textured Mars Bronze GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-350-LW50-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 5000K OB Gunmetal Grey GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-350-LW50-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 350mA 5000K OB Custom RAL GSA,E3 LED Engine,350mA (5W LED),Cool White (5000K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-350-LW50-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-350-LW30-OB,4.4
E3 500mA 2200K NB Black GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-500-LW22-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2200K NB White GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-500-LW22-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2200K NB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW22-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2200K NB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW22-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2200K NB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW22-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2200K NB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW22-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2200K NB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-500-LW22-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2200K MB Black GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-500-LW22-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2200K MB White GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-500-LW22-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2200K MB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW22-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2200K MB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW22-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2200K MB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW22-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2200K MB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW22-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2200K MB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-500-LW22-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2200K WB Black GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-500-LW22-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2200K WB White GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-500-LW22-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2200K WB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW22-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2200K WB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW22-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2200K WB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW22-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2200K WB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW22-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2200K WB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-500-LW22-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2200K WWB Black GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-500-LW22-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2200K WWB White GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-500-LW22-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2200K WWB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW22-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2200K WWB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW22-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2200K WWB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW22-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2200K WWB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW22-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2200K WWB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-500-LW22-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2200K OB Black GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-500-LW22-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2200K OB White GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-500-LW22-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2200K OB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW22-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2200K OB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW22-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2200K OB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW22-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2200K OB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW22-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2200K OB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-500-LW22-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2700K NB Black GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-500-LW27-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2700K NB White GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-500-LW27-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2700K NB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW27-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2700K NB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW27-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2700K NB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW27-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2700K NB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW27-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2700K NB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-500-LW27-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 2700K MB Black GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-500-LW27-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2700K MB White GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-500-LW27-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2700K MB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW27-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2700K MB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW27-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2700K MB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW27-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2700K MB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW27-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2700K MB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-500-LW27-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 2700K WB Black GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-500-LW27-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2700K WB White GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-500-LW27-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2700K WB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW27-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2700K WB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW27-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2700K WB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW27-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2700K WB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW27-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2700K WB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-500-LW27-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 2700K WWB Black GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-500-LW27-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2700K WWB White GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-500-LW27-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2700K WWB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW27-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2700K WWB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW27-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2700K WWB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW27-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2700K WWB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW27-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2700K WWB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-500-LW27-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 2700K OB Black GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-500-LW27-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2700K OB White GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-500-LW27-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2700K OB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW27-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2700K OB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW27-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2700K OB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW27-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2700K OB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW27-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 2700K OB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-500-LW27-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 3000K NB Black GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-500-LW30-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 3000K NB White GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-500-LW30-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 3000K NB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW30-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 3000K NB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW30-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 3000K NB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW30-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 3000K NB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW30-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 3000K NB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-500-LW30-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 3000K MB Black GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-500-LW30-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 3000K MB White GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-500-LW30-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 3000K MB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW30-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 3000K MB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW30-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 3000K MB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW30-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 3000K MB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW30-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 3000K MB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-500-LW30-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 3000K WB Black GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-500-LW30-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 3000K WB White GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-500-LW30-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 3000K WB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW30-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 3000K WB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW30-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 3000K WB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW30-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 3000K WB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW30-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 3000K WB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-500-LW30-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 3000K WWB Black GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-500-LW30-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 3000K WWB White GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-500-LW30-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 3000K WWB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW30-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 3000K WWB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW30-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 3000K WWB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW30-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 3000K WWB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW30-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 3000K WWB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-500-LW30-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 3000K OB Black GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-500-LW30-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 3000K OB White GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-500-LW30-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 3000K OB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW30-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 3000K OB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW30-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 3000K OB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW30-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 3000K OB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW30-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 3000K OB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Warm White (3000K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-500-LW30-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 4000K NB Black GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-500-LW40-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 4000K NB White GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-500-LW40-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 4000K NB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW40-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 4000K NB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW40-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 4000K NB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW40-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 4000K NB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW40-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 4000K NB Custom RAL GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-500-LW40-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 4000K MB Black GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-500-LW40-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 4000K MB White GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,19° Medium,Powder Coat White (RAL 9016),LD10238-E3-500-LW40-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 4000K MB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW40-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 4000K MB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW40-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 4000K MB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW40-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 4000K MB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW40-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 4000K MB Custom RAL GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,19° Medium,Powder Coat RAL (TBD),LD10238-E3-500-LW40-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 4000K WB Black GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-500-LW40-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 4000K WB White GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,34° Wide,Powder Coat White (RAL 9016),LD10238-E3-500-LW40-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 4000K WB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW40-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 4000K WB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW40-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 4000K WB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW40-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 4000K WB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW40-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 4000K WB Custom RAL GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,34° Wide,Powder Coat RAL (TBD),LD10238-E3-500-LW40-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 4000K WWB Black GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-500-LW40-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 4000K WWB White GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-500-LW40-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 4000K WWB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW40-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 4000K WWB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW40-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 4000K WWB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW40-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 4000K WWB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW40-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 4000K WWB Custom RAL GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-500-LW40-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 4000K OB Black GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-500-LW40-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 4000K OB White GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-500-LW40-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 4000K OB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW40-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 4000K OB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW40-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 4000K OB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW40-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 4000K OB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW40-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 4000K OB Custom RAL GSA,E3 LED Engine,500mA (7W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-500-LW40-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 5000K NB Black GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-500-LW50-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 5000K NB White GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-500-LW50-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 5000K NB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW50-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 5000K NB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW50-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 5000K NB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW50-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 5000K NB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW50-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 5000K NB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-500-LW50-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-NB,6.4
E3 500mA 5000K MB Black GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-500-LW50-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 5000K MB White GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-500-LW50-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 5000K MB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW50-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 5000K MB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW50-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 5000K MB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW50-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 5000K MB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW50-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 5000K MB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-500-LW50-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-MB,6.4
E3 500mA 5000K WB Black GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-500-LW50-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 5000K WB White GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-500-LW50-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 5000K WB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW50-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 5000K WB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW50-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 5000K WB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW50-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 5000K WB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW50-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 5000K WB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-500-LW50-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WB,6.4
E3 500mA 5000K WWB Black GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-500-LW50-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 5000K WWB White GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-500-LW50-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 5000K WWB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW50-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 5000K WWB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW50-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 5000K WWB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW50-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 5000K WWB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW50-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 5000K WWB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-500-LW50-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-WWB,6.4
E3 500mA 5000K OB Black GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-500-LW50-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 5000K OB White GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-500-LW50-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 5000K OB Classic Bronze GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-500-LW50-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 5000K OB Textured Fir Green GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-500-LW50-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 5000K OB Textured Mars Bronze GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-500-LW50-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 5000K OB Gunmetal Grey GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-500-LW50-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 500mA 5000K OB Custom RAL GSA,E3 LED Engine,500mA (7W LED),Cool White (5000K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-500-LW50-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-E3-500-LW30-OB,6.4
E3 700mA 2200K NB Black GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-700-LW22-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2200K NB White GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-700-LW22-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2200K NB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW22-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2200K NB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW22-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2200K NB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW22-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2200K NB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW22-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2200K NB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-700-LW22-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2200K MB Black GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-700-LW22-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2200K MB White GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-700-LW22-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2200K MB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW22-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2200K MB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW22-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2200K MB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW22-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2200K MB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW22-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2200K MB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-700-LW22-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2200K WB Black GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-700-LW22-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2200K WB White GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-700-LW22-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2200K WB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW22-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2200K WB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW22-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2200K WB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW22-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2200K WB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW22-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2200K WB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-700-LW22-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2200K WWB Black GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-700-LW22-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2200K WWB White GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-700-LW22-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2200K WWB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW22-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2200K WWB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW22-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2200K WWB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW22-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2200K WWB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW22-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2200K WWB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-700-LW22-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2200K OB Black GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-700-LW22-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2200K OB White GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-700-LW22-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2200K OB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW22-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2200K OB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW22-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2200K OB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW22-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2200K OB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW22-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2200K OB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Super Warm White (2200K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-700-LW22-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2700K NB Black GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-700-LW27-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2700K NB White GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-700-LW27-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2700K NB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW27-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2700K NB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW27-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2700K NB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW27-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2700K NB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW27-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2700K NB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-700-LW27-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 2700K MB Black GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-700-LW27-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2700K MB White GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-700-LW27-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2700K MB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW27-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2700K MB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW27-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2700K MB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW27-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2700K MB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW27-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2700K MB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-700-LW27-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 2700K WB Black GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-700-LW27-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2700K WB White GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-700-LW27-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2700K WB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW27-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2700K WB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW27-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2700K WB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW27-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2700K WB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW27-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2700K WB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-700-LW27-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 2700K WWB Black GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-700-LW27-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2700K WWB White GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-700-LW27-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2700K WWB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW27-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2700K WWB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW27-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2700K WWB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW27-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2700K WWB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW27-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2700K WWB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-700-LW27-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 2700K OB Black GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-700-LW27-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2700K OB White GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-700-LW27-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2700K OB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW27-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2700K OB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW27-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2700K OB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW27-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2700K OB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW27-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 2700K OB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Extra Warm White (2700K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-700-LW27-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 3000K NB Black GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-700-LW30-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 3000K NB White GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-700-LW30-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 3000K NB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW30-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 3000K NB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW30-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 3000K NB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW30-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 3000K NB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW30-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 3000K NB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-700-LW30-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 3000K MB Black GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-700-LW30-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 3000K MB White GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-700-LW30-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 3000K MB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW30-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 3000K MB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW30-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 3000K MB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW30-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 3000K MB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW30-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 3000K MB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-700-LW30-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 3000K WB Black GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-700-LW30-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 3000K WB White GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-700-LW30-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 3000K WB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW30-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 3000K WB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW30-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 3000K WB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW30-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 3000K WB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW30-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 3000K WB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-700-LW30-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 3000K WWB Black GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-700-LW30-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 3000K WWB White GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-700-LW30-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 3000K WWB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW30-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 3000K WWB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW30-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 3000K WWB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW30-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 3000K WWB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW30-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 3000K WWB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-700-LW30-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 3000K OB Black GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-700-LW30-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 3000K OB White GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-700-LW30-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 3000K OB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW30-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 3000K OB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW30-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 3000K OB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW30-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 3000K OB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW30-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 3000K OB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Warm White (3000K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-700-LW30-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 4000K NB Black GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-700-LW40-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 4000K NB White GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-700-LW40-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 4000K NB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW40-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 4000K NB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW40-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 4000K NB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW40-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 4000K NB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW40-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 4000K NB Custom RAL GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-700-LW40-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 4000K MB Black GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-700-LW40-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 4000K MB White GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,19° Medium,Powder Coat White (RAL 9016),LD10238-E3-700-LW40-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 4000K MB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW40-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 4000K MB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW40-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 4000K MB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW40-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 4000K MB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW40-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 4000K MB Custom RAL GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,19° Medium,Powder Coat RAL (TBD),LD10238-E3-700-LW40-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 4000K WB Black GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-700-LW40-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 4000K WB White GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,34° Wide,Powder Coat White (RAL 9016),LD10238-E3-700-LW40-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 4000K WB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW40-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 4000K WB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW40-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 4000K WB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW40-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 4000K WB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW40-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 4000K WB Custom RAL GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,34° Wide,Powder Coat RAL (TBD),LD10238-E3-700-LW40-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 4000K WWB Black GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-700-LW40-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 4000K WWB White GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-700-LW40-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 4000K WWB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW40-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 4000K WWB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW40-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 4000K WWB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW40-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 4000K WWB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW40-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 4000K WWB Custom RAL GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-700-LW40-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 4000K OB Black GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-700-LW40-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 4000K OB White GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-700-LW40-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 4000K OB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW40-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 4000K OB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW40-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 4000K OB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW40-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 4000K OB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW40-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 4000K OB Custom RAL GSA,E3 LED Engine,700mA (10W LED),White (4000K) - on request,15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-700-LW40-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 5000K NB Black GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Black (RAL 9005),LD10238-E3-700-LW50-NB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 5000K NB White GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),12° Narrow Spot,Powder Coat White (RAL 9016),LD10238-E3-700-LW50-NB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 5000K NB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW50-NB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 5000K NB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW50-NB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 5000K NB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW50-NB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 5000K NB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),12° Narrow Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW50-NB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 5000K NB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),12° Narrow Spot,Powder Coat RAL (TBD),LD10238-E3-700-LW50-NB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-NB,9.2
E3 700mA 5000K MB Black GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),19° Medium,Powder Coat Black (RAL 9005),LD10238-E3-700-LW50-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 5000K MB White GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),19° Medium,Powder Coat White (RAL 9016),LD10238-E3-700-LW50-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 5000K MB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),19° Medium,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW50-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 5000K MB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),19° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW50-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 5000K MB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),19° Medium,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW50-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 5000K MB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),19° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW50-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 5000K MB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),19° Medium,Powder Coat RAL (TBD),LD10238-E3-700-LW50-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-MB,9.2
E3 700mA 5000K WB Black GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),34° Wide,Powder Coat Black (RAL 9005),LD10238-E3-700-LW50-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 5000K WB White GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),34° Wide,Powder Coat White (RAL 9016),LD10238-E3-700-LW50-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 5000K WB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),34° Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW50-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 5000K WB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),34° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW50-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 5000K WB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),34° Wide,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW50-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 5000K WB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),34° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW50-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 5000K WB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),34° Wide,Powder Coat RAL (TBD),LD10238-E3-700-LW50-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WB,9.2
E3 700mA 5000K WWB Black GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),54° Extra Wide,Powder Coat Black (RAL 9005),LD10238-E3-700-LW50-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 5000K WWB White GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),54° Extra Wide,Powder Coat White (RAL 9016),LD10238-E3-700-LW50-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 5000K WWB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),54° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW50-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 5000K WWB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),54° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW50-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 5000K WWB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),54° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW50-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 5000K WWB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),54° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW50-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 5000K WWB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),54° Extra Wide,Powder Coat RAL (TBD),LD10238-E3-700-LW50-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-WWB,9.2
E3 700mA 5000K OB Black GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Black (RAL 9005),LD10238-E3-700-LW50-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 5000K OB White GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),15° x 49° Oval,Powder Coat White (RAL 9016),LD10238-E3-700-LW50-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 5000K OB Classic Bronze GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Classic Bronze (YM262E),LD10238-E3-700-LW50-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 5000K OB Textured Fir Green GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-E3-700-LW50-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 5000K OB Textured Mars Bronze GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Textured Mars Bronze,LD10238-E3-700-LW50-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 5000K OB Gunmetal Grey GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),15° x 49° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-E3-700-LW50-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
E3 700mA 5000K OB Custom RAL GSA,E3 LED Engine,700mA (10W LED),Cool White (5000K),15° x 49° Oval,Powder Coat RAL (TBD),LD10238-E3-700-LW50-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),85,NICHIA E3 LED,-20°C to 50°C,LightGraphix_IES_LD10238 : LD10238-E3-700-LW30-OB,9.2
N1 350mA 2200K MSB Black GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-350-LW22-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2200K MSB White GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-350-LW22-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2200K MSB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW22-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2200K MSB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW22-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2200K MSB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW22-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2200K MSB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW22-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2200K MSB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-350-LW22-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2200K MB Black GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-350-LW22-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2200K MB White GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-350-LW22-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2200K MB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW22-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2200K MB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW22-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2200K MB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW22-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2200K MB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW22-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2200K MB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-350-LW22-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2200K WB Black GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-350-LW22-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2200K WB White GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-350-LW22-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2200K WB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW22-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2200K WB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW22-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2200K WB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW22-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2200K WB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW22-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2200K WB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-350-LW22-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2200K WWB Black GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-350-LW22-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2200K WWB White GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-350-LW22-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2200K WWB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW22-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2200K WWB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW22-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2200K WWB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW22-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2200K WWB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW22-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2200K WWB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-350-LW22-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2200K OB Black GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-350-LW22-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2200K OB White GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-350-LW22-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2200K OB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW22-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2200K OB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW22-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2200K OB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW22-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2200K OB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW22-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2200K OB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-350-LW22-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2700K MSB Black GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-350-LW27-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2700K MSB White GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-350-LW27-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2700K MSB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW27-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2700K MSB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW27-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2700K MSB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW27-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2700K MSB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW27-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2700K MSB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-350-LW27-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 2700K MB Black GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-350-LW27-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2700K MB White GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-350-LW27-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2700K MB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW27-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2700K MB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW27-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2700K MB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW27-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2700K MB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW27-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2700K MB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-350-LW27-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 2700K WB Black GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-350-LW27-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2700K WB White GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-350-LW27-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2700K WB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW27-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2700K WB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW27-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2700K WB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW27-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2700K WB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW27-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2700K WB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-350-LW27-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 2700K WWB Black GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-350-LW27-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2700K WWB White GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-350-LW27-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2700K WWB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW27-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2700K WWB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW27-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2700K WWB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW27-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2700K WWB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW27-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2700K WWB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-350-LW27-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 2700K OB Black GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-350-LW27-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2700K OB White GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-350-LW27-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2700K OB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW27-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2700K OB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW27-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2700K OB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW27-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2700K OB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW27-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 2700K OB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-350-LW27-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 3000K MSB Black GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-350-LW30-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 3000K MSB White GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-350-LW30-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 3000K MSB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW30-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 3000K MSB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW30-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 3000K MSB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW30-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 3000K MSB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW30-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 3000K MSB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-350-LW30-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 3000K MB Black GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-350-LW30-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 3000K MB White GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-350-LW30-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 3000K MB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW30-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 3000K MB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW30-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 3000K MB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW30-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 3000K MB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW30-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 3000K MB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-350-LW30-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 3000K WB Black GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-350-LW30-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 3000K WB White GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-350-LW30-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 3000K WB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW30-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 3000K WB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW30-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 3000K WB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW30-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 3000K WB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW30-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 3000K WB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-350-LW30-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 3000K WWB Black GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-350-LW30-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 3000K WWB White GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-350-LW30-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 3000K WWB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW30-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 3000K WWB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW30-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 3000K WWB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW30-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 3000K WWB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW30-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 3000K WWB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-350-LW30-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 3000K OB Black GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-350-LW30-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 3000K OB White GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-350-LW30-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 3000K OB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW30-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 3000K OB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW30-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 3000K OB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW30-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 3000K OB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW30-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 3000K OB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Warm White (3000K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-350-LW30-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 4000K MSB Black GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-350-LW40-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 4000K MSB White GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-350-LW40-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 4000K MSB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW40-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 4000K MSB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW40-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 4000K MSB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW40-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 4000K MSB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW40-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 4000K MSB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-350-LW40-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 4000K MB Black GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-350-LW40-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 4000K MB White GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,35° Medium,Powder Coat White (RAL 9016),LD10238-N1-350-LW40-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 4000K MB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW40-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 4000K MB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW40-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 4000K MB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW40-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 4000K MB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW40-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 4000K MB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,35° Medium,Powder Coat RAL (TBD),LD10238-N1-350-LW40-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 4000K WB Black GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-350-LW40-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 4000K WB White GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,46° Wide,Powder Coat White (RAL 9016),LD10238-N1-350-LW40-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 4000K WB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW40-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 4000K WB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW40-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 4000K WB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW40-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 4000K WB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW40-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 4000K WB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,46° Wide,Powder Coat RAL (TBD),LD10238-N1-350-LW40-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 4000K WWB Black GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-350-LW40-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 4000K WWB White GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-350-LW40-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 4000K WWB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW40-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 4000K WWB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW40-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 4000K WWB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW40-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 4000K WWB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW40-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 4000K WWB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-350-LW40-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 4000K OB Black GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-350-LW40-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 4000K OB White GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-350-LW40-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 4000K OB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW40-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 4000K OB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW40-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 4000K OB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW40-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 4000K OB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW40-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 4000K OB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-350-LW40-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 5000K MSB Black GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-350-LW50-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 5000K MSB White GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-350-LW50-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 5000K MSB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW50-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 5000K MSB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW50-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 5000K MSB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW50-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 5000K MSB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW50-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 5000K MSB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-350-LW50-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MSB,6.4
N1 350mA 5000K MB Black GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-350-LW50-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 5000K MB White GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-350-LW50-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 5000K MB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW50-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 5000K MB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW50-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 5000K MB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW50-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 5000K MB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW50-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 5000K MB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-350-LW50-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-MB,6.4
N1 350mA 5000K WB Black GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-350-LW50-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 5000K WB White GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-350-LW50-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 5000K WB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW50-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 5000K WB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW50-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 5000K WB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW50-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 5000K WB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW50-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 5000K WB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-350-LW50-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WB,6.4
N1 350mA 5000K WWB Black GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-350-LW50-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 5000K WWB White GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-350-LW50-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 5000K WWB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW50-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 5000K WWB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW50-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 5000K WWB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW50-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 5000K WWB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW50-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 5000K WWB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-350-LW50-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-WWB,6.4
N1 350mA 5000K OB Black GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-350-LW50-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 5000K OB White GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-350-LW50-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 5000K OB Classic Bronze GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-350-LW50-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 5000K OB Textured Fir Green GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-350-LW50-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 5000K OB Textured Mars Bronze GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-350-LW50-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 5000K OB Gunmetal Grey GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-350-LW50-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 350mA 5000K OB Custom RAL GSA,N1 COB LED Engine,350mA (7W LED),Cool White (5000K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-350-LW50-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-350-LW30-OB,6.4
N1 500mA 2200K MSB Black GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-500-LW22-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2200K MSB White GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-500-LW22-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2200K MSB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW22-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2200K MSB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW22-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2200K MSB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW22-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2200K MSB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW22-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2200K MSB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-500-LW22-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2200K MB Black GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-500-LW22-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2200K MB White GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-500-LW22-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2200K MB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW22-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2200K MB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW22-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2200K MB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW22-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2200K MB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW22-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2200K MB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-500-LW22-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2200K WB Black GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-500-LW22-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2200K WB White GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-500-LW22-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2200K WB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW22-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2200K WB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW22-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2200K WB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW22-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2200K WB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW22-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2200K WB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-500-LW22-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2200K WWB Black GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-500-LW22-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2200K WWB White GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-500-LW22-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2200K WWB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW22-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2200K WWB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW22-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2200K WWB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW22-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2200K WWB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW22-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2200K WWB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-500-LW22-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2200K OB Black GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-500-LW22-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2200K OB White GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-500-LW22-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2200K OB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW22-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2200K OB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW22-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2200K OB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW22-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2200K OB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW22-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2200K OB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-500-LW22-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2700K MSB Black GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-500-LW27-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2700K MSB White GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-500-LW27-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2700K MSB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW27-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2700K MSB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW27-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2700K MSB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW27-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2700K MSB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW27-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2700K MSB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-500-LW27-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 2700K MB Black GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-500-LW27-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2700K MB White GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-500-LW27-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2700K MB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW27-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2700K MB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW27-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2700K MB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW27-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2700K MB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW27-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2700K MB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-500-LW27-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 2700K WB Black GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-500-LW27-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2700K WB White GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-500-LW27-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2700K WB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW27-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2700K WB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW27-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2700K WB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW27-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2700K WB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW27-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2700K WB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-500-LW27-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 2700K WWB Black GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-500-LW27-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2700K WWB White GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-500-LW27-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2700K WWB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW27-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2700K WWB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW27-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2700K WWB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW27-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2700K WWB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW27-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2700K WWB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-500-LW27-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 2700K OB Black GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-500-LW27-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2700K OB White GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-500-LW27-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2700K OB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW27-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2700K OB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW27-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2700K OB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW27-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2700K OB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW27-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 2700K OB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-500-LW27-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 3000K MSB Black GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-500-LW30-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 3000K MSB White GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-500-LW30-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 3000K MSB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW30-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 3000K MSB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW30-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 3000K MSB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW30-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 3000K MSB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW30-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 3000K MSB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-500-LW30-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 3000K MB Black GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-500-LW30-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 3000K MB White GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-500-LW30-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 3000K MB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW30-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 3000K MB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW30-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 3000K MB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW30-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 3000K MB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW30-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 3000K MB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-500-LW30-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 3000K WB Black GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-500-LW30-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 3000K WB White GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-500-LW30-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 3000K WB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW30-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 3000K WB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW30-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 3000K WB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW30-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 3000K WB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW30-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 3000K WB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-500-LW30-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 3000K WWB Black GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-500-LW30-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 3000K WWB White GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-500-LW30-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 3000K WWB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW30-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 3000K WWB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW30-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 3000K WWB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW30-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 3000K WWB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW30-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 3000K WWB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-500-LW30-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 3000K OB Black GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-500-LW30-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 3000K OB White GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-500-LW30-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 3000K OB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW30-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 3000K OB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW30-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 3000K OB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW30-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 3000K OB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW30-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 3000K OB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Warm White (3000K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-500-LW30-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 4000K MSB Black GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-500-LW40-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 4000K MSB White GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-500-LW40-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 4000K MSB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW40-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 4000K MSB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW40-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 4000K MSB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW40-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 4000K MSB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW40-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 4000K MSB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-500-LW40-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 4000K MB Black GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-500-LW40-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 4000K MB White GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,35° Medium,Powder Coat White (RAL 9016),LD10238-N1-500-LW40-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 4000K MB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW40-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 4000K MB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW40-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 4000K MB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW40-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 4000K MB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW40-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 4000K MB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,35° Medium,Powder Coat RAL (TBD),LD10238-N1-500-LW40-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 4000K WB Black GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-500-LW40-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 4000K WB White GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,46° Wide,Powder Coat White (RAL 9016),LD10238-N1-500-LW40-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 4000K WB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW40-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 4000K WB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW40-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 4000K WB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW40-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 4000K WB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW40-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 4000K WB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,46° Wide,Powder Coat RAL (TBD),LD10238-N1-500-LW40-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 4000K WWB Black GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-500-LW40-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 4000K WWB White GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-500-LW40-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 4000K WWB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW40-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 4000K WWB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW40-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 4000K WWB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW40-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 4000K WWB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW40-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 4000K WWB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-500-LW40-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 4000K OB Black GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-500-LW40-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 4000K OB White GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-500-LW40-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 4000K OB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW40-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 4000K OB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW40-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 4000K OB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW40-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 4000K OB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW40-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 4000K OB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-500-LW40-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 5000K MSB Black GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-500-LW50-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 5000K MSB White GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-500-LW50-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 5000K MSB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW50-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 5000K MSB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW50-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 5000K MSB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW50-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 5000K MSB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW50-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 5000K MSB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-500-LW50-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MSB,9.3
N1 500mA 5000K MB Black GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-500-LW50-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 5000K MB White GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-500-LW50-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 5000K MB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW50-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 5000K MB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW50-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 5000K MB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW50-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 5000K MB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW50-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 5000K MB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-500-LW50-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-MB,9.3
N1 500mA 5000K WB Black GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-500-LW50-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 5000K WB White GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-500-LW50-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 5000K WB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW50-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 5000K WB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW50-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 5000K WB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW50-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 5000K WB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW50-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 5000K WB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-500-LW50-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WB,9.3
N1 500mA 5000K WWB Black GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-500-LW50-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 5000K WWB White GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-500-LW50-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 5000K WWB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW50-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 5000K WWB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW50-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 5000K WWB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW50-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 5000K WWB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW50-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 5000K WWB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-500-LW50-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-WWB,9.3
N1 500mA 5000K OB Black GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-500-LW50-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 5000K OB White GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-500-LW50-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 5000K OB Classic Bronze GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-500-LW50-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 5000K OB Textured Fir Green GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-500-LW50-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 5000K OB Textured Mars Bronze GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-500-LW50-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 5000K OB Gunmetal Grey GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-500-LW50-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 500mA 5000K OB Custom RAL GSA,N1 COB LED Engine,500mA (10W LED),Cool White (5000K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-500-LW50-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 55°C,LightGraphix_IES_LD10238 : LD10238-N1-500-LW30-OB,9.3
N1 700mA 2200K MSB Black GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-700-LW22-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2200K MSB White GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-700-LW22-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2200K MSB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW22-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2200K MSB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW22-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2200K MSB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW22-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2200K MSB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW22-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2200K MSB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-700-LW22-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2200K MB Black GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-700-LW22-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2200K MB White GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-700-LW22-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2200K MB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW22-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2200K MB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW22-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2200K MB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW22-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2200K MB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW22-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2200K MB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-700-LW22-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2200K WB Black GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-700-LW22-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2200K WB White GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-700-LW22-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2200K WB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW22-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2200K WB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW22-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2200K WB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW22-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2200K WB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW22-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2200K WB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-700-LW22-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2200K WWB Black GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-700-LW22-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2200K WWB White GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-700-LW22-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2200K WWB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW22-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2200K WWB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW22-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2200K WWB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW22-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2200K WWB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW22-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2200K WWB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-700-LW22-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2200K OB Black GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-700-LW22-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2200K OB White GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-700-LW22-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2200K OB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW22-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2200K OB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW22-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2200K OB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW22-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2200K OB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW22-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2200K OB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Super Warm White (2200K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-700-LW22-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2700K MSB Black GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-700-LW27-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2700K MSB White GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-700-LW27-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2700K MSB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW27-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2700K MSB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW27-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2700K MSB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW27-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2700K MSB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW27-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2700K MSB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-700-LW27-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 2700K MB Black GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-700-LW27-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2700K MB White GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-700-LW27-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2700K MB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW27-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2700K MB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW27-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2700K MB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW27-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2700K MB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW27-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2700K MB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-700-LW27-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 2700K WB Black GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-700-LW27-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2700K WB White GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-700-LW27-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2700K WB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW27-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2700K WB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW27-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2700K WB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW27-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2700K WB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW27-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2700K WB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-700-LW27-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 2700K WWB Black GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-700-LW27-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2700K WWB White GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-700-LW27-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2700K WWB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW27-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2700K WWB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW27-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2700K WWB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW27-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2700K WWB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW27-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2700K WWB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-700-LW27-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 2700K OB Black GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-700-LW27-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2700K OB White GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-700-LW27-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2700K OB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW27-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2700K OB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW27-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2700K OB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW27-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2700K OB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW27-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 2700K OB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Extra Warm White (2700K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-700-LW27-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 3000K MSB Black GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-700-LW30-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 3000K MSB White GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-700-LW30-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 3000K MSB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW30-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 3000K MSB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW30-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 3000K MSB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW30-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 3000K MSB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW30-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 3000K MSB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-700-LW30-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 3000K MB Black GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-700-LW30-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 3000K MB White GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-700-LW30-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 3000K MB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW30-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 3000K MB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW30-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 3000K MB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW30-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 3000K MB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW30-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 3000K MB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-700-LW30-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 3000K WB Black GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-700-LW30-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 3000K WB White GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-700-LW30-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 3000K WB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW30-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 3000K WB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW30-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 3000K WB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW30-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 3000K WB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW30-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 3000K WB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-700-LW30-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 3000K WWB Black GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-700-LW30-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 3000K WWB White GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-700-LW30-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 3000K WWB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW30-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 3000K WWB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW30-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 3000K WWB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW30-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 3000K WWB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW30-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 3000K WWB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-700-LW30-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 3000K OB Black GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-700-LW30-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 3000K OB White GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-700-LW30-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 3000K OB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW30-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 3000K OB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW30-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 3000K OB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW30-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 3000K OB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW30-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 3000K OB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Warm White (3000K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-700-LW30-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 4000K MSB Black GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-700-LW40-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 4000K MSB White GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-700-LW40-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 4000K MSB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW40-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 4000K MSB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW40-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 4000K MSB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW40-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 4000K MSB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW40-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 4000K MSB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-700-LW40-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 4000K MB Black GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-700-LW40-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 4000K MB White GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,35° Medium,Powder Coat White (RAL 9016),LD10238-N1-700-LW40-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 4000K MB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW40-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 4000K MB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW40-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 4000K MB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW40-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 4000K MB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW40-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 4000K MB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,35° Medium,Powder Coat RAL (TBD),LD10238-N1-700-LW40-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 4000K WB Black GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-700-LW40-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 4000K WB White GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,46° Wide,Powder Coat White (RAL 9016),LD10238-N1-700-LW40-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 4000K WB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW40-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 4000K WB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW40-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 4000K WB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW40-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 4000K WB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW40-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 4000K WB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,46° Wide,Powder Coat RAL (TBD),LD10238-N1-700-LW40-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 4000K WWB Black GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-700-LW40-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 4000K WWB White GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-700-LW40-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 4000K WWB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW40-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 4000K WWB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW40-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 4000K WWB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW40-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 4000K WWB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW40-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 4000K WWB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-700-LW40-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 4000K OB Black GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-700-LW40-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 4000K OB White GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-700-LW40-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 4000K OB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW40-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 4000K OB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW40-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 4000K OB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW40-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 4000K OB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW40-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 4000K OB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),White (4000K) - on request,22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-700-LW40-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 5000K MSB Black GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),25° Medium Spot,Powder Coat Black (RAL 9005),LD10238-N1-700-LW50-MSB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 5000K MSB White GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),25° Medium Spot,Powder Coat White (RAL 9016),LD10238-N1-700-LW50-MSB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 5000K MSB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),25° Medium Spot,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW50-MSB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 5000K MSB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),25° Medium Spot,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW50-MSB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 5000K MSB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),25° Medium Spot,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW50-MSB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 5000K MSB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),25° Medium Spot,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW50-MSB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 5000K MSB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),25° Medium Spot,Powder Coat RAL (TBD),LD10238-N1-700-LW50-MSB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MSB,13.3
N1 700mA 5000K MB Black GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),35° Medium,Powder Coat Black (RAL 9005),LD10238-N1-700-LW50-MB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 5000K MB White GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),35° Medium,Powder Coat White (RAL 9016),LD10238-N1-700-LW50-MB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 5000K MB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),35° Medium,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW50-MB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 5000K MB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),35° Medium,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW50-MB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 5000K MB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),35° Medium,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW50-MB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 5000K MB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),35° Medium,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW50-MB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 5000K MB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),35° Medium,Powder Coat RAL (TBD),LD10238-N1-700-LW50-MB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-MB,13.3
N1 700mA 5000K WB Black GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),46° Wide,Powder Coat Black (RAL 9005),LD10238-N1-700-LW50-WB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 5000K WB White GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),46° Wide,Powder Coat White (RAL 9016),LD10238-N1-700-LW50-WB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 5000K WB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),46° Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW50-WB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 5000K WB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),46° Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW50-WB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 5000K WB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),46° Wide,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW50-WB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 5000K WB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),46° Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW50-WB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 5000K WB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),46° Wide,Powder Coat RAL (TBD),LD10238-N1-700-LW50-WB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WB,13.3
N1 700mA 5000K WWB Black GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),65° Extra Wide,Powder Coat Black (RAL 9005),LD10238-N1-700-LW50-WWB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 5000K WWB White GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),65° Extra Wide,Powder Coat White (RAL 9016),LD10238-N1-700-LW50-WWB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 5000K WWB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),65° Extra Wide,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW50-WWB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 5000K WWB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),65° Extra Wide,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW50-WWB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 5000K WWB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),65° Extra Wide,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW50-WWB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 5000K WWB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),65° Extra Wide,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW50-WWB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 5000K WWB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),65° Extra Wide,Powder Coat RAL (TBD),LD10238-N1-700-LW50-WWB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-WWB,13.3
N1 700mA 5000K OB Black GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Black (RAL 9005),LD10238-N1-700-LW50-OB/Black/GSA,Powder Coat Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 5000K OB White GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),22° x 43° Oval,Powder Coat White (RAL 9016),LD10238-N1-700-LW50-OB/White/GSA,Powder Coat White (RAL 9016),LightGraphix_Finish_PowderCoat_White,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 5000K OB Classic Bronze GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Classic Bronze (YM262E),LD10238-N1-700-LW50-OB/Classic Bronze/GSA,Powder Coat Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 5000K OB Textured Fir Green GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Textured Fir Green (RAL 6009),LD10238-N1-700-LW50-OB/Textured Fir Green/GSA,Powder Coat Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 5000K OB Textured Mars Bronze GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Textured Mars Bronze,LD10238-N1-700-LW50-OB/Textured Mars Bronze/GSA,Powder Coat Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 5000K OB Gunmetal Grey GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),22° x 43° Oval,Powder Coat Gunmetal Grey (RAL 7021),LD10238-N1-700-LW50-OB/Gunmetal Grey/GSA,Powder Coat Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
N1 700mA 5000K OB Custom RAL GSA,N1 COB LED Engine,700mA (14W LED),Cool White (5000K),22° x 43° Oval,Powder Coat RAL (TBD),LD10238-N1-700-LW50-OB/Custom RAL/GSA,Powder Coat RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),93,CREE N1 LED,-20°C to 35°C,LightGraphix_IES_LD10238 : LD10238-N1-700-LW30-OB,13.3
