,Light Engine##OTHER##,Drive Current##OTHER##,LED Colour##OTHER##,LED Spacing##OTHER##,Beam Angle##OTHER##,Model##OTHER##,Colour##OTHER##,Finish Material##OTHER##,Control IES##OTHER##,MFG_LightSource##OTHER##,MFG_TemperatureRating##OTHER##,MFG_Wattage##ELECTRICAL_WATTAGE##WATTS
900mm 50mm Spacing 2200K 350mA Narrow Beam Black,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-350/LW22/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Narrow Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-350/LW22/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Narrow Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-350/LW22/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Narrow Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-350/LW22/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Narrow Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-350/LW22/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-350/LW22/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Narrow Beam White,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-350/LW22/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Medium Beam Black,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-350/LW22/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Medium Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-350/LW22/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Medium Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-350/LW22/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Medium Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-350/LW22/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Medium Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-350/LW22/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Medium Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-350/LW22/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Medium Beam White,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-350/LW22/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Wide Beam Black,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-350/LW22/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Wide Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-350/LW22/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Wide Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-350/LW22/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Wide Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-350/LW22/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Wide Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-350/LW22/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Wide Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-350/LW22/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Wide Beam White,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-350/LW22/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Extra Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Extra Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Extra Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2200K 350mA Extra Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 75mm Spacing 2200K 350mA Narrow Beam Black,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-350/LW22/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Narrow Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-350/LW22/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Narrow Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-350/LW22/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Narrow Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-350/LW22/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Narrow Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-350/LW22/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-350/LW22/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Narrow Beam White,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-350/LW22/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Medium Beam Black,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-350/LW22/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Medium Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-350/LW22/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Medium Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-350/LW22/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Medium Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-350/LW22/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Medium Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-350/LW22/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Medium Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-350/LW22/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Medium Beam White,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-350/LW22/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Wide Beam Black,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-350/LW22/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Wide Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-350/LW22/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Wide Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-350/LW22/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Wide Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-350/LW22/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Wide Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-350/LW22/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Wide Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-350/LW22/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Wide Beam White,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-350/LW22/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW22/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Extra Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Extra Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Extra Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2200K 350mA Extra Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW22/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 50mm Spacing 2700K 350mA Narrow Beam Black,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-350/LW27/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Narrow Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-350/LW27/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Narrow Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-350/LW27/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Narrow Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-350/LW27/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Narrow Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-350/LW27/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-350/LW27/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Narrow Beam White,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-350/LW27/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Medium Beam Black,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-350/LW27/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Medium Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-350/LW27/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Medium Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-350/LW27/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Medium Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-350/LW27/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Medium Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-350/LW27/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Medium Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-350/LW27/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Medium Beam White,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-350/LW27/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Wide Beam Black,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-350/LW27/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Wide Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-350/LW27/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Wide Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-350/LW27/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Wide Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-350/LW27/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Wide Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-350/LW27/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Wide Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-350/LW27/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Wide Beam White,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-350/LW27/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Extra Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Extra Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Extra Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 2700K 350mA Extra Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 75mm Spacing 2700K 350mA Narrow Beam Black,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-350/LW27/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Narrow Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-350/LW27/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Narrow Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-350/LW27/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Narrow Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-350/LW27/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Narrow Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-350/LW27/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-350/LW27/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Narrow Beam White,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-350/LW27/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Medium Beam Black,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-350/LW27/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Medium Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-350/LW27/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Medium Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-350/LW27/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Medium Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-350/LW27/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Medium Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-350/LW27/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Medium Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-350/LW27/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Medium Beam White,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-350/LW27/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Wide Beam Black,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-350/LW27/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Wide Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-350/LW27/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Wide Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-350/LW27/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Wide Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-350/LW27/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Wide Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-350/LW27/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Wide Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-350/LW27/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Wide Beam White,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-350/LW27/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW27/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Extra Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Extra Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Extra Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 2700K 350mA Extra Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW27/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 50mm Spacing 3000K 350mA Narrow Beam Black,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-350/LW30/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Narrow Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-350/LW30/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Narrow Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-350/LW30/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Narrow Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-350/LW30/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Narrow Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-350/LW30/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-350/LW30/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Narrow Beam White,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-350/LW30/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Medium Beam Black,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-350/LW30/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Medium Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-350/LW30/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Medium Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-350/LW30/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Medium Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-350/LW30/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Medium Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-350/LW30/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Medium Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-350/LW30/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Medium Beam White,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-350/LW30/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Wide Beam Black,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-350/LW30/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Wide Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-350/LW30/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Wide Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-350/LW30/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Wide Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-350/LW30/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Wide Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-350/LW30/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Wide Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-350/LW30/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Wide Beam White,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-350/LW30/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Extra Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Extra Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Extra Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 3000K 350mA Extra Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 75mm Spacing 3000K 350mA Narrow Beam Black,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-350/LW30/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Narrow Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-350/LW30/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Narrow Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-350/LW30/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Narrow Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-350/LW30/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Narrow Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-350/LW30/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-350/LW30/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Narrow Beam White,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-350/LW30/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Medium Beam Black,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-350/LW30/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Medium Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-350/LW30/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Medium Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-350/LW30/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Medium Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-350/LW30/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Medium Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-350/LW30/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Medium Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-350/LW30/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Medium Beam White,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-350/LW30/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Wide Beam Black,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-350/LW30/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Wide Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-350/LW30/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Wide Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-350/LW30/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Wide Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-350/LW30/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Wide Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-350/LW30/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Wide Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-350/LW30/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Wide Beam White,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-350/LW30/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW30/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Extra Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Extra Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Extra Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 3000K 350mA Extra Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW30/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 50mm Spacing 4000K 350mA Narrow Beam Black,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-350/LW40/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Narrow Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-350/LW40/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Narrow Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-350/LW40/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Narrow Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-350/LW40/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Narrow Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-350/LW40/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-350/LW40/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Narrow Beam White,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-350/LW40/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Medium Beam Black,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-350/LW40/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Medium Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-350/LW40/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Medium Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-350/LW40/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Medium Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-350/LW40/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Medium Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-350/LW40/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Medium Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-350/LW40/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Medium Beam White,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-350/LW40/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Wide Beam Black,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-350/LW40/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Wide Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-350/LW40/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Wide Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-350/LW40/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Wide Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-350/LW40/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Wide Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-350/LW40/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Wide Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-350/LW40/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Wide Beam White,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-350/LW40/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Oval Beam White,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Extra Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Extra Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Extra Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 4000K 350mA Extra Oval Beam White,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 75mm Spacing 4000K 350mA Narrow Beam Black,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-350/LW40/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Narrow Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-350/LW40/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Narrow Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-350/LW40/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Narrow Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-350/LW40/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Narrow Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-350/LW40/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-350/LW40/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Narrow Beam White,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-350/LW40/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Medium Beam Black,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-350/LW40/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Medium Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-350/LW40/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Medium Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-350/LW40/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Medium Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-350/LW40/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Medium Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-350/LW40/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Medium Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-350/LW40/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Medium Beam White,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-350/LW40/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Wide Beam Black,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-350/LW40/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Wide Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-350/LW40/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Wide Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-350/LW40/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Wide Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-350/LW40/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Wide Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-350/LW40/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Wide Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-350/LW40/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Wide Beam White,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-350/LW40/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Oval Beam White,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-350/LW40/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Extra Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Extra Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Extra Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 4000K 350mA Extra Oval Beam White,Linear C1 Engine,350mA (1.2W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW40/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 50mm Spacing 5000K 350mA Narrow Beam Black,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-350/LW50/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Narrow Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-350/LW50/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Narrow Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-350/LW50/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Narrow Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-350/LW50/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Narrow Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-350/LW50/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-350/LW50/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Narrow Beam White,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-350/LW50/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Medium Beam Black,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-350/LW50/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Medium Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-350/LW50/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Medium Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-350/LW50/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Medium Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-350/LW50/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Medium Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-350/LW50/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Medium Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-350/LW50/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Medium Beam White,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-350/LW50/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Wide Beam Black,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-350/LW50/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Wide Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-350/LW50/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Wide Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-350/LW50/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Wide Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-350/LW50/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Wide Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-350/LW50/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Wide Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-350/LW50/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Wide Beam White,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-350/LW50/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Extra Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Extra Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Extra Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 50mm Spacing 5000K 350mA Extra Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,19.8
900mm 75mm Spacing 5000K 350mA Narrow Beam Black,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-350/LW50/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Narrow Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-350/LW50/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Narrow Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-350/LW50/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Narrow Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-350/LW50/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Narrow Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-350/LW50/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-350/LW50/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Narrow Beam White,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-350/LW50/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Medium Beam Black,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-350/LW50/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Medium Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-350/LW50/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Medium Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-350/LW50/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Medium Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-350/LW50/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Medium Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-350/LW50/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Medium Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-350/LW50/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Medium Beam White,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-350/LW50/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Wide Beam Black,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-350/LW50/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Wide Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-350/LW50/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Wide Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-350/LW50/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Wide Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-350/LW50/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Wide Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-350/LW50/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Wide Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-350/LW50/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Wide Beam White,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-350/LW50/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-350/LW50/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Extra Oval Beam Black,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Extra Oval Beam Classic Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Extra Oval Beam RAL TBD,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 75mm Spacing 5000K 350mA Extra Oval Beam White,Linear C1 Engine,350mA (1.2W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-350/LW50/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-350-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 55°C,13.2
900mm 50mm Spacing 2200K 500mA Narrow Beam Black,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-500/LW22/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Narrow Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-500/LW22/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Narrow Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-500/LW22/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Narrow Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-500/LW22/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Narrow Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-500/LW22/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-500/LW22/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Narrow Beam White,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-500/LW22/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Medium Beam Black,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-500/LW22/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Medium Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-500/LW22/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Medium Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-500/LW22/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Medium Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-500/LW22/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Medium Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-500/LW22/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Medium Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-500/LW22/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Medium Beam White,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-500/LW22/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Wide Beam Black,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-500/LW22/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Wide Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-500/LW22/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Wide Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-500/LW22/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Wide Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-500/LW22/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Wide Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-500/LW22/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Wide Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-500/LW22/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Wide Beam White,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-500/LW22/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Extra Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Extra Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Extra Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2200K 500mA Extra Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 75mm Spacing 2200K 500mA Narrow Beam Black,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-500/LW22/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Narrow Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-500/LW22/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Narrow Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-500/LW22/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Narrow Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-500/LW22/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Narrow Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-500/LW22/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-500/LW22/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Narrow Beam White,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-500/LW22/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Medium Beam Black,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-500/LW22/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Medium Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-500/LW22/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Medium Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-500/LW22/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Medium Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-500/LW22/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Medium Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-500/LW22/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Medium Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-500/LW22/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Medium Beam White,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-500/LW22/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Wide Beam Black,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-500/LW22/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Wide Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-500/LW22/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Wide Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-500/LW22/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Wide Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-500/LW22/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Wide Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-500/LW22/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Wide Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-500/LW22/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Wide Beam White,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-500/LW22/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW22/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Extra Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Extra Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Extra Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2200K 500mA Extra Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW22/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 50mm Spacing 2700K 500mA Narrow Beam Black,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-500/LW27/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Narrow Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-500/LW27/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Narrow Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-500/LW27/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Narrow Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-500/LW27/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Narrow Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-500/LW27/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-500/LW27/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Narrow Beam White,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-500/LW27/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Medium Beam Black,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-500/LW27/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Medium Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-500/LW27/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Medium Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-500/LW27/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Medium Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-500/LW27/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Medium Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-500/LW27/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Medium Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-500/LW27/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Medium Beam White,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-500/LW27/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Wide Beam Black,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-500/LW27/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Wide Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-500/LW27/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Wide Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-500/LW27/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Wide Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-500/LW27/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Wide Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-500/LW27/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Wide Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-500/LW27/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Wide Beam White,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-500/LW27/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Extra Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Extra Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Extra Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 2700K 500mA Extra Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 75mm Spacing 2700K 500mA Narrow Beam Black,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-500/LW27/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Narrow Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-500/LW27/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Narrow Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-500/LW27/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Narrow Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-500/LW27/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Narrow Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-500/LW27/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-500/LW27/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Narrow Beam White,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-500/LW27/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Medium Beam Black,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-500/LW27/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Medium Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-500/LW27/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Medium Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-500/LW27/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Medium Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-500/LW27/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Medium Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-500/LW27/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Medium Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-500/LW27/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Medium Beam White,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-500/LW27/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Wide Beam Black,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-500/LW27/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Wide Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-500/LW27/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Wide Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-500/LW27/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Wide Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-500/LW27/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Wide Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-500/LW27/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Wide Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-500/LW27/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Wide Beam White,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-500/LW27/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW27/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Extra Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Extra Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Extra Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 2700K 500mA Extra Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW27/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 50mm Spacing 3000K 500mA Narrow Beam Black,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-500/LW30/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Narrow Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-500/LW30/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Narrow Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-500/LW30/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Narrow Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-500/LW30/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Narrow Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-500/LW30/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-500/LW30/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Narrow Beam White,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-500/LW30/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Medium Beam Black,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-500/LW30/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Medium Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-500/LW30/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Medium Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-500/LW30/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Medium Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-500/LW30/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Medium Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-500/LW30/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Medium Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-500/LW30/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Medium Beam White,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-500/LW30/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Wide Beam Black,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-500/LW30/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Wide Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-500/LW30/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Wide Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-500/LW30/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Wide Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-500/LW30/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Wide Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-500/LW30/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Wide Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-500/LW30/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Wide Beam White,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-500/LW30/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Extra Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Extra Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Extra Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 3000K 500mA Extra Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 75mm Spacing 3000K 500mA Narrow Beam Black,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-500/LW30/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Narrow Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-500/LW30/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Narrow Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-500/LW30/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Narrow Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-500/LW30/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Narrow Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-500/LW30/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-500/LW30/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Narrow Beam White,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-500/LW30/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Medium Beam Black,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-500/LW30/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Medium Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-500/LW30/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Medium Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-500/LW30/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Medium Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-500/LW30/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Medium Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-500/LW30/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Medium Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-500/LW30/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Medium Beam White,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-500/LW30/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Wide Beam Black,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-500/LW30/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Wide Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-500/LW30/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Wide Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-500/LW30/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Wide Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-500/LW30/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Wide Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-500/LW30/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Wide Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-500/LW30/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Wide Beam White,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-500/LW30/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW30/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Extra Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Extra Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Extra Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 3000K 500mA Extra Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW30/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 50mm Spacing 4000K 500mA Narrow Beam Black,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-500/LW40/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Narrow Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-500/LW40/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Narrow Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-500/LW40/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Narrow Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-500/LW40/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Narrow Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-500/LW40/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-500/LW40/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Narrow Beam White,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-500/LW40/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Medium Beam Black,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-500/LW40/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Medium Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-500/LW40/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Medium Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-500/LW40/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Medium Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-500/LW40/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Medium Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-500/LW40/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Medium Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-500/LW40/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Medium Beam White,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-500/LW40/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Wide Beam Black,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-500/LW40/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Wide Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-500/LW40/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Wide Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-500/LW40/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Wide Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-500/LW40/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Wide Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-500/LW40/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Wide Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-500/LW40/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Wide Beam White,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-500/LW40/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Oval Beam White,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Extra Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Extra Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Extra Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 4000K 500mA Extra Oval Beam White,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 75mm Spacing 4000K 500mA Narrow Beam Black,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-500/LW40/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Narrow Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-500/LW40/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Narrow Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-500/LW40/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Narrow Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-500/LW40/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Narrow Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-500/LW40/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-500/LW40/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Narrow Beam White,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-500/LW40/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Medium Beam Black,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-500/LW40/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Medium Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-500/LW40/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Medium Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-500/LW40/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Medium Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-500/LW40/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Medium Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-500/LW40/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Medium Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-500/LW40/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Medium Beam White,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-500/LW40/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Wide Beam Black,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-500/LW40/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Wide Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-500/LW40/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Wide Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-500/LW40/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Wide Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-500/LW40/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Wide Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-500/LW40/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Wide Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-500/LW40/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Wide Beam White,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-500/LW40/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Oval Beam White,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-500/LW40/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Extra Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Extra Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Extra Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 4000K 500mA Extra Oval Beam White,Linear C1 Engine,500mA (1.7W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW40/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 50mm Spacing 5000K 500mA Narrow Beam Black,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-500/LW50/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Narrow Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-500/LW50/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Narrow Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-500/LW50/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Narrow Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-500/LW50/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Narrow Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-500/LW50/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-500/LW50/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Narrow Beam White,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-500/LW50/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Medium Beam Black,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-500/LW50/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Medium Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-500/LW50/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Medium Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-500/LW50/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Medium Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-500/LW50/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Medium Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-500/LW50/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Medium Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-500/LW50/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Medium Beam White,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-500/LW50/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Wide Beam Black,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-500/LW50/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Wide Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-500/LW50/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Wide Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-500/LW50/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Wide Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-500/LW50/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Wide Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-500/LW50/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Wide Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-500/LW50/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Wide Beam White,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-500/LW50/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Extra Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Extra Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Extra Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 50mm Spacing 5000K 500mA Extra Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,28.8
900mm 75mm Spacing 5000K 500mA Narrow Beam Black,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-500/LW50/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Narrow Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-500/LW50/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Narrow Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-500/LW50/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Narrow Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-500/LW50/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Narrow Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-500/LW50/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-500/LW50/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Narrow Beam White,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-500/LW50/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Medium Beam Black,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-500/LW50/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Medium Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-500/LW50/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Medium Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-500/LW50/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Medium Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-500/LW50/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Medium Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-500/LW50/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Medium Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-500/LW50/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Medium Beam White,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-500/LW50/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Wide Beam Black,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-500/LW50/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Wide Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-500/LW50/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Wide Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-500/LW50/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Wide Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-500/LW50/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Wide Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-500/LW50/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Wide Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-500/LW50/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Wide Beam White,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-500/LW50/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-500/LW50/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Extra Oval Beam Black,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Extra Oval Beam Classic Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Extra Oval Beam RAL TBD,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 75mm Spacing 5000K 500mA Extra Oval Beam White,Linear C1 Engine,500mA (1.7W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-500/LW50/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-500-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 50°C,19.2
900mm 50mm Spacing 2200K 700mA Narrow Beam Black,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-700/LW22/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Narrow Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-700/LW22/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Narrow Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-700/LW22/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Narrow Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-700/LW22/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Narrow Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-700/LW22/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-700/LW22/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Narrow Beam White,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Narrow Beam (12°),LD34-C1-700/LW22/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Medium Beam Black,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-700/LW22/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Medium Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-700/LW22/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Medium Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-700/LW22/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Medium Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-700/LW22/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Medium Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-700/LW22/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Medium Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-700/LW22/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Medium Beam White,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Medium Beam (31°),LD34-C1-700/LW22/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Wide Beam Black,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-700/LW22/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Wide Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-700/LW22/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Wide Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-700/LW22/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Wide Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-700/LW22/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Wide Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-700/LW22/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Wide Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-700/LW22/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Wide Beam White,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Wide Beam (48°),LD34-C1-700/LW22/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Extra Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Extra Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Extra Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2200K 700mA Extra Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 75mm Spacing 2200K 700mA Narrow Beam Black,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-700/LW22/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Narrow Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-700/LW22/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Narrow Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-700/LW22/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Narrow Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-700/LW22/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Narrow Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-700/LW22/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-700/LW22/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Narrow Beam White,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Narrow Beam (12°),LD34-C1-700/LW22/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Medium Beam Black,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-700/LW22/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Medium Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-700/LW22/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Medium Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-700/LW22/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Medium Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-700/LW22/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Medium Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-700/LW22/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Medium Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-700/LW22/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Medium Beam White,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Medium Beam (31°),LD34-C1-700/LW22/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Wide Beam Black,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-700/LW22/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Wide Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-700/LW22/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Wide Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-700/LW22/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Wide Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-700/LW22/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Wide Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-700/LW22/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Wide Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-700/LW22/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Wide Beam White,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Wide Beam (48°),LD34-C1-700/LW22/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW22/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Extra Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Extra Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Extra Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2200K 700mA Extra Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Super Warm White (2200K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW22/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW22-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 50mm Spacing 2700K 700mA Narrow Beam Black,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-700/LW27/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Narrow Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-700/LW27/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Narrow Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-700/LW27/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Narrow Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-700/LW27/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Narrow Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-700/LW27/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-700/LW27/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Narrow Beam White,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Narrow Beam (12°),LD34-C1-700/LW27/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Medium Beam Black,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-700/LW27/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Medium Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-700/LW27/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Medium Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-700/LW27/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Medium Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-700/LW27/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Medium Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-700/LW27/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Medium Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-700/LW27/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Medium Beam White,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Medium Beam (31°),LD34-C1-700/LW27/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Wide Beam Black,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-700/LW27/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Wide Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-700/LW27/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Wide Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-700/LW27/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Wide Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-700/LW27/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Wide Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-700/LW27/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Wide Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-700/LW27/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Wide Beam White,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Wide Beam (48°),LD34-C1-700/LW27/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Extra Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Extra Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Extra Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 2700K 700mA Extra Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 75mm Spacing 2700K 700mA Narrow Beam Black,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-700/LW27/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Narrow Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-700/LW27/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Narrow Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-700/LW27/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Narrow Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-700/LW27/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Narrow Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-700/LW27/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-700/LW27/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Narrow Beam White,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Narrow Beam (12°),LD34-C1-700/LW27/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Medium Beam Black,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-700/LW27/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Medium Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-700/LW27/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Medium Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-700/LW27/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Medium Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-700/LW27/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Medium Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-700/LW27/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Medium Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-700/LW27/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Medium Beam White,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Medium Beam (31°),LD34-C1-700/LW27/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Wide Beam Black,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-700/LW27/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Wide Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-700/LW27/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Wide Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-700/LW27/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Wide Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-700/LW27/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Wide Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-700/LW27/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Wide Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-700/LW27/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Wide Beam White,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Wide Beam (48°),LD34-C1-700/LW27/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW27/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Extra Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Extra Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Extra Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 2700K 700mA Extra Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Extra Warm White (2700K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW27/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW27-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 50mm Spacing 3000K 700mA Narrow Beam Black,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-700/LW30/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Narrow Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-700/LW30/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Narrow Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-700/LW30/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Narrow Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-700/LW30/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Narrow Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-700/LW30/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-700/LW30/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Narrow Beam White,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Narrow Beam (12°),LD34-C1-700/LW30/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Medium Beam Black,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-700/LW30/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Medium Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-700/LW30/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Medium Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-700/LW30/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Medium Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-700/LW30/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Medium Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-700/LW30/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Medium Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-700/LW30/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Medium Beam White,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Medium Beam (31°),LD34-C1-700/LW30/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Wide Beam Black,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-700/LW30/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Wide Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-700/LW30/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Wide Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-700/LW30/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Wide Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-700/LW30/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Wide Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-700/LW30/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Wide Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-700/LW30/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Wide Beam White,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Wide Beam (48°),LD34-C1-700/LW30/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Extra Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Extra Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Extra Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 3000K 700mA Extra Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 75mm Spacing 3000K 700mA Narrow Beam Black,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-700/LW30/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Narrow Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-700/LW30/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Narrow Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-700/LW30/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Narrow Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-700/LW30/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Narrow Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-700/LW30/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-700/LW30/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Narrow Beam White,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Narrow Beam (12°),LD34-C1-700/LW30/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Medium Beam Black,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-700/LW30/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Medium Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-700/LW30/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Medium Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-700/LW30/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Medium Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-700/LW30/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Medium Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-700/LW30/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Medium Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-700/LW30/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Medium Beam White,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Medium Beam (31°),LD34-C1-700/LW30/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Wide Beam Black,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-700/LW30/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Wide Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-700/LW30/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Wide Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-700/LW30/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Wide Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-700/LW30/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Wide Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-700/LW30/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Wide Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-700/LW30/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Wide Beam White,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Wide Beam (48°),LD34-C1-700/LW30/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW30/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Extra Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Extra Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Extra Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 3000K 700mA Extra Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Warm White (3000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW30/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW30-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 50mm Spacing 4000K 700mA Narrow Beam Black,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-700/LW40/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Narrow Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-700/LW40/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Narrow Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-700/LW40/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Narrow Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-700/LW40/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Narrow Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-700/LW40/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-700/LW40/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Narrow Beam White,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Narrow Beam (12°),LD34-C1-700/LW40/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Medium Beam Black,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-700/LW40/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Medium Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-700/LW40/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Medium Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-700/LW40/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Medium Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-700/LW40/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Medium Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-700/LW40/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Medium Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-700/LW40/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Medium Beam White,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Medium Beam (31°),LD34-C1-700/LW40/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Wide Beam Black,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-700/LW40/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Wide Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-700/LW40/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Wide Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-700/LW40/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Wide Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-700/LW40/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Wide Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-700/LW40/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Wide Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-700/LW40/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Wide Beam White,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Wide Beam (48°),LD34-C1-700/LW40/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Oval Beam White,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Extra Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Extra Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Extra Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 4000K 700mA Extra Oval Beam White,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 75mm Spacing 4000K 700mA Narrow Beam Black,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-700/LW40/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Narrow Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-700/LW40/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Narrow Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-700/LW40/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Narrow Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-700/LW40/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Narrow Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-700/LW40/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-700/LW40/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Narrow Beam White,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Narrow Beam (12°),LD34-C1-700/LW40/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Medium Beam Black,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-700/LW40/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Medium Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-700/LW40/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Medium Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-700/LW40/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Medium Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-700/LW40/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Medium Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-700/LW40/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Medium Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-700/LW40/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Medium Beam White,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Medium Beam (31°),LD34-C1-700/LW40/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Wide Beam Black,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-700/LW40/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Wide Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-700/LW40/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Wide Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-700/LW40/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Wide Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-700/LW40/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Wide Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-700/LW40/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Wide Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-700/LW40/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Wide Beam White,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Wide Beam (48°),LD34-C1-700/LW40/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Oval Beam White,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Oval Beam (12° x 36°),LD34-C1-700/LW40/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Extra Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Extra Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Extra Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 4000K 700mA Extra Oval Beam White,Linear C1 Engine,700mA (2.4W LED),White (4000K) - on request,75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW40/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW40-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 50mm Spacing 5000K 700mA Narrow Beam Black,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-700/LW50/50/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Narrow Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-700/LW50/50/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Narrow Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-700/LW50/50/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Narrow Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-700/LW50/50/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Narrow Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-700/LW50/50/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-700/LW50/50/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Narrow Beam White,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Narrow Beam (12°),LD34-C1-700/LW50/50/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Medium Beam Black,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-700/LW50/50/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Medium Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-700/LW50/50/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Medium Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-700/LW50/50/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Medium Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-700/LW50/50/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Medium Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-700/LW50/50/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Medium Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-700/LW50/50/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Medium Beam White,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Medium Beam (31°),LD34-C1-700/LW50/50/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Wide Beam Black,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-700/LW50/50/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Wide Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-700/LW50/50/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Wide Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-700/LW50/50/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Wide Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-700/LW50/50/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Wide Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-700/LW50/50/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Wide Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-700/LW50/50/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Wide Beam White,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Wide Beam (48°),LD34-C1-700/LW50/50/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/50/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/50/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/50/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/50/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/50/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/50/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/50/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Extra Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/50/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Extra Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/50/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/50/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Extra Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/50/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/50/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/50/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 50mm Spacing 5000K 700mA Extra Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),50mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/50/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-50-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,41.4
900mm 75mm Spacing 5000K 700mA Narrow Beam Black,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-700/LW50/75/NB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Narrow Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-700/LW50/75/NB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Narrow Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-700/LW50/75/NB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Narrow Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-700/LW50/75/NB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Narrow Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-700/LW50/75/NB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Narrow Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-700/LW50/75/NB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Narrow Beam White,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Narrow Beam (12°),LD34-C1-700/LW50/75/NB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-NB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Medium Beam Black,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-700/LW50/75/MB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Medium Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-700/LW50/75/MB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Medium Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-700/LW50/75/MB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Medium Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-700/LW50/75/MB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Medium Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-700/LW50/75/MB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Medium Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-700/LW50/75/MB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Medium Beam White,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Medium Beam (31°),LD34-C1-700/LW50/75/MB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-900-MB,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Wide Beam Black,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-700/LW50/75/WB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Wide Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-700/LW50/75/WB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Wide Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-700/LW50/75/WB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Wide Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-700/LW50/75/WB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Wide Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-700/LW50/75/WB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Wide Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-700/LW50/75/WB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Wide Beam White,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Wide Beam (48°),LD34-C1-700/LW50/75/WB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-WB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/75/OB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/75/OB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/75/OB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/75/OB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/75/OB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/75/OB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Oval Beam (12° x 36°),LD34-C1-700/LW50/75/OB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-OB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Extra Oval Beam Black,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/75/EOB/Black/SC/900,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Extra Oval Beam Classic Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/75/EOB/Classic Bronze/SC/900,Paint Finish Classic Bronze (YM262E),LightGraphix_Finish_PowderCoat_ClassicBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Extra Oval Beam Gunmetal Grey,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/75/EOB/Gunmetal Grey/SC/900,Paint Finish Gunmetal Grey (RAL 7021),LightGraphix_Finish_PowderCoat_GunmetalGrey,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Extra Oval Beam RAL TBD,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/75/EOB/RAL/SC/900,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Extra Oval Beam Textured Fir Green,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/75/EOB/Textured Fir Green/SC/900,Paint Finish Textured Fir Green (RAL 6009),LightGraphix_Finish_PowderCoat_TexturedFirGreen,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Extra Oval Beam Textured Mars Bronze,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/75/EOB/Textured Mars Bronze/SC/900,Paint Finish Textured Mars Bronze,LightGraphix_Finish_PowderCoat_TexturedMarsBronze,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
900mm 75mm Spacing 5000K 700mA Extra Oval Beam White,Linear C1 Engine,700mA (2.4W LED),Cool White (5000K),75mm,Extra Oval Beam (15° x 60°),LD34-C1-700/LW50/75/EOB/White/SC/900,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,LightGraphix_IES_LD34_900 : LD34-C1-700-LW50-75-EOB-900,NICHIA Linear C1 Engine,-20°C to 45°C,27.6
